E-Mobility Product Catalog 2026
CNVera
CNVera is an exporter based in Haikou, Hainan, China. Our industrial range covers specialty lubricants and, as this catalog shows, personal electric mobility: electric dirt bikes, electric bikes and electric scooters for leisure, sport and urban commuting. We supply distributors, retailers and fleet buyers worldwide, with export packing, mixed-model container loading and documentation support.
Range overview
Electric dirt bikes: Wish 01 SE, Wish 01 EEC, Wish 01 mini, Wish 01 plus, Wish 01 pro
Electric bikes: T01, T01 pro
Electric scooters: G2 MAX, G2 booster, M2 pro, G5
Accessories: Holder 01 hitch-mounted carrier rack
Certifications and quality
The products in this catalog are tested and certified for their target markets, including CE, RoHS and FCC requirements, with SGS test reports available on request. The range is covered by more than 40 utility model patents. Full documentation is supplied with export orders on request.
Specifications below follow the manufacturer datasheets and are subject to change without notice. Contact us for current pricing, MOQ and OEM options.
1. Electric Dirt Bikes
Wish 01 SE
Electric dirt bike for off-road leisure riding, aluminum alloy frame, hydraulic brakes front and rear.
	Parameter
	Specification

	Motor
	2 kW (rated power 1.2 kW)

	Battery
	48 V 20.8 Ah (22.5 Ah / 27 Ah options)

	Charge voltage
	54.6 V

	Max speed
	55 km/h

	Mileage
	50 km

	Tire
	14 inch (front) / 12 inch (rear), pneumatic

	Max load
	120 kg

	Max slope
	30%

	Brake
	Hydraulic brake

	Display
	LCD: speed, gear, battery, range

	Light system
	Without headlight

	Material
	Aluminum alloy

	Shock absorption
	(front) Hydraulic shock absorber; (rear) adjustable hydraulic nitrogen shock absorber

	Charge time
	7–8 hrs

	Foldable
	No

	Seat
	Yes

	Suitable age
	16–50 years old

	NW / GW
	48 / 57 kg

	Carton size
	1300 x 300 x 770 mm

	Unfolded size
	1510 x 780 x 1000 mm

	Loading qty
	249 pcs / 40HQ (normal packing); 213 pcs / 40HQ (overall packing)



Wish 01 EEC
Road-equipped version of the Wish 01 with full lighting (headlight, tail light and turning lights) for markets that require it.
	Parameter
	Specification

	Motor
	2 kW (rated power 1.2 kW)

	Battery
	48 V 20.8 Ah

	Charge voltage
	54.6 V

	Max speed
	55 km/h

	Mileage
	50 km

	Tire
	14 inch (front) / 12 inch (rear), pneumatic

	Max load
	120 kg

	Max slope
	30%

	Brake
	Hydraulic brake

	Display
	LCD: speed, gear, battery, range

	Light system
	Headlight / tail light / turning light

	Material
	Aluminum alloy

	Shock absorption
	(front) Hydraulic shock absorber; (rear) adjustable hydraulic nitrogen shock absorber

	Charge time
	7–8 hrs

	Foldable
	No

	Seat
	Yes

	Suitable age
	16–50 years old

	NW / GW
	48 / 55 kg

	Carton size
	1276 x 276 x 745 mm

	Unfolded size
	1510 x 780 x 1000 mm

	Loading qty
	104 pcs / 20GP; 249 pcs / 40HQ



Wish 01 mini
Junior electric dirt bike, sized and powered for younger riders.
	Parameter
	Specification

	Motor
	1 kW (rated power 0.5 kW)

	Battery
	48 V 10 Ah

	Max speed
	35 km/h (22 mph)

	Mileage
	35 km (50 kg loading, under 25 km/h)

	Tire
	10 inch

	Max load
	100 kg

	Brake
	Disc brake + electric brake

	Material
	6061 aluminum alloy

	Shock absorption
	(front) Hydraulic forks, wheel travel 140 mm; (rear) spring suspension

	Charge time
	5 hours

	Seat height
	580 mm

	Height
	740 mm

	NW / GW
	25 / 30 kg

	Drivetrain
	Hub

	Wheelbase
	830 mm

	Ground clearance
	220 mm



Wish 01 plus
	Parameter
	Specification

	Motor
	3 kW (rated power 1.5 kW)

	Battery
	52 V 27 Ah

	Max speed
	72 km/h (45 mph)

	Mileage
	80 km (65 kg loading, under 35 km/h)

	Tire
	14 (front) / 12 (rear) inch, or 17 (front) / 14 (rear) inch

	Max load
	150 kg (265 lbs)

	Brake
	Hydraulic brake

	Material
	6061 aluminum alloy

	Shock absorption
	(front) Hydraulic forks, wheel travel 160 mm; (rear) adjustable hydraulic nitrogen shock absorber

	Charge time
	6 hours

	Seat height
	800 mm

	Height
	1020 mm

	NW / GW
	58 / 63 kg

	Drivetrain
	Chain drive

	Wheelbase
	1100 mm

	Ground clearance
	280 mm



Wish 01 pro
Flagship of the Wish 01 line, with a 60 V 35 Ah LG-cell battery and 5 kW peak power.
	Parameter
	Specification

	Motor
	5 kW (rated power 2.5 kW)

	Battery
	60 V 35 Ah (LG cells)

	Max speed
	80 km/h (50 mph)

	Mileage
	80 km (65 kg loading, under 35 km/h)

	Tire
	17 (front) / 14 (rear) inch

	Max load
	150 kg (330 lbs)

	Brake
	Hydraulic brake

	Material
	6061 aluminum alloy

	Shock absorption
	(front) Hydraulic forks, wheel travel 160 mm; (rear) adjustable hydraulic nitrogen shock absorber

	Charge time
	7 hours

	Seat height
	820 mm

	Height
	1020 mm

	NW / GW
	56 / 61 kg

	Drivetrain
	Chain drive

	Wheelbase
	1100 mm

	Ground clearance
	280 mm



2. Electric Bikes
T01
Moto-style electric bike with 20-inch pneumatic tires and full suspension.
	Parameter
	Specification

	Motor
	1 kW (rated power 0.5 kW)

	Battery
	48 V 15 Ah

	Charge voltage
	54.6 V

	Max speed
	48 km/h

	Mileage
	60 km (65 kg loading, under 35 km/h)

	Tire
	20 inch, pneumatic

	Max load
	150 kg

	Max slope
	30%

	Brake
	Hydraulic brake

	Display
	LCD: speed, gear, battery, range

	Light system
	Headlight

	Material
	Aluminum alloy

	Shock absorption
	(front) Oil shock absorber; (rear) air shock absorber

	Charge time
	7–8 hrs

	Foldable
	No

	Seat
	Yes

	Suitable age
	16–50 years old

	NW / GW
	38 / 42 kg

	Carton size
	1440 x 300 x 820 mm

	Unfolded size
	1710 x 650 x 1110 mm

	Loading qty
	72 pcs / 20GP; 185 pcs / 40HQ



T01 pro
	Parameter
	Specification

	Motor
	3000 W

	Battery
	52 V 25 Ah

	Charge voltage
	58.8 V

	Max speed
	70 km/h

	Mileage
	100 km (65 kg loading, under 35 km/h)

	Tire
	20 inch, pneumatic

	Max load
	150 kg

	Max slope
	35%

	Brake
	Hydraulic brake

	Display
	LCD: speed, gear, battery, range

	Light system
	Headlight

	Material
	Aluminum alloy

	Shock absorption
	(front) Oil shock absorber; (rear) air shock absorber

	Charge time
	8–9 hrs

	Foldable
	No

	Seat
	Yes

	Suitable age
	16–50 years old

	NW / GW
	50 / 55 kg

	Carton size
	1195 x 275 x 490 mm

	Unfolded size
	1190 x 575 x 1150 mm

	Loading qty
	176 pcs / 40HQ



3. Electric Scooters
G2 MAX
Foldable off-road style electric scooter, single motor.
	Parameter
	Specification

	Motor
	1050 W – 1200 W

	Battery
	48 V 18 Ah

	Charge voltage
	54.6 V

	Max speed
	53 km/h

	Mileage
	45–60 km

	Tire
	10 inch, vacuum tyre

	Max load
	150 kg

	Max slope
	30%

	Brake
	Disc brake

	Display
	LCD: speed, gear, battery, range

	Light system
	Headlight / side light / tail light

	Material
	Aluminum alloy

	Shock absorption
	Spring shock absorber

	Charge time
	9–10 hrs

	Foldable
	Yes

	Seat
	No

	Suitable age
	16–50 years old

	NW / GW
	26.95 / 30.95 kg

	Carton size
	1190 x 270 x 600 mm

	Unfolded size
	1190 x 240 x 1320 mm

	Loading qty
	128 pcs / 20GP; 350 pcs / 40HQ



G2 booster
Dual-motor version of the G2 for stronger climbing and acceleration.
	Parameter
	Specification

	Motor
	900 W – 1000 W x 2

	Battery
	52 V 22.5 Ah

	Charge voltage
	58.8 V

	Max speed
	60–65 km/h

	Mileage
	40–65 km

	Tire
	10 inch, pneumatic

	Max load
	150 kg

	Max slope
	40%

	Brake
	Disc brake

	Display
	LCD: speed, gear, battery, range

	Light system
	Headlight / side light / tail light

	Material
	Aluminum alloy

	Shock absorption
	Spring shock absorber

	Charge time
	10–11 hrs

	Foldable
	Yes

	Seat
	No

	Suitable age
	16–50 years old

	NW / GW
	32 / 37 kg

	Carton size
	1190 x 270 x 600 mm

	Unfolded size
	1190 x 270 x 1270 mm

	Loading qty
	128 pcs / 20GP; 350 pcs / 40HQ



M2 pro
Lightweight foldable commuter scooter for last-mile city travel.
	Parameter
	Specification

	Motor
	350 W

	Battery
	36 V 7.5 Ah / 36 V 10 Ah

	Charge voltage
	42 V

	Max speed
	30 km/h

	Mileage
	25–30 km

	Tire
	8.5 inch, pneumatic

	Max load
	120 kg

	Max slope
	15%

	Brake
	Disc brake

	Display
	LCD: speed, gear, battery, range

	Light system
	Headlight / tail light

	Material
	Aluminum alloy

	Shock absorption
	Spring shock absorber

	Charge time
	4–5 hrs

	Foldable
	Yes

	Seat
	No

	Suitable age
	16–50 years old

	NW / GW
	15.5 / 18 kg

	Carton size
	1110 x 205 x 425 mm

	Unfolded size
	1110 x 500 x 1100 mm

	Loading qty
	300 pcs / 20GP; 700 pcs / 40HQ



G5
	Parameter
	Specification

	Motor
	500 W

	Battery
	48 V 16 Ah

	Charge voltage
	54.6 V

	Max speed
	35 km/h

	Mileage
	50 km

	Tire
	10 inch, pneumatic

	Max load
	120 kg

	Max slope
	15%

	Brake
	Disc brake

	Display
	LCD: speed, gear, battery, range

	Light system
	Headlight / turning light / side light / tail light

	Material
	Aluminum alloy

	Shock absorption
	Spring shock absorber

	Charge time
	7–8 hrs

	Foldable
	Yes

	Seat
	No

	Suitable age
	16–50 years old

	NW / GW
	23 / 26.5 kg

	Carton size
	1185 x 270 x 490 mm

	Unfolded size
	1185 x 270 x 490 mm

	Loading qty
	165 pcs / 20GP; 400 pcs / 40HQ



4. Accessories
Holder 01
Hitch-mounted carrier rack for transporting one motorcycle, e-bike or electric dirt bike on a vehicle with a compatible 2-inch hitch receiver. Usage: unlock the two locks, unfold the carrier rack, release the straps and push the motorcycle down.
	Parameter
	Specification

	Designed for
	Transporting one motorcycle, e-bike or electric dirt bike on a vehicle with a compatible 2-inch hitch receiver

	Suitable for
	Wheelbase range 103 to 128 cm (40.5 to 50.4 in)

	Product size
	1420 x 600 x 850 mm

	Material
	6061 aluminum alloy and reinforced steel

	Max load
	265 lbs

	Net weight
	71.5 lbs

	Gross weight
	76 lbs

	Packing size
	1030 x 540 x 260 mm



Contact
Email: gosanya@gmail.com
WhatsApp: +86 139 2516 5566 (wa.me/8613925165566)
Address: Room 1201, Block C, Shimao Center, Longhua District, Haikou, Hainan, China
We reply within 24 hours.




